{"text_format":"3","workbook":"xlsx","n_sheets":5,"sheets":["2026年","204个档次","63个品目","37个小类","18个大类"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"2026年","index":0,"n_rows":206,"n_cols":8,"rows_kept":206,"merged":[[0,0,0,7],[49,7,54,7]]}
["云南省2024—2026年农业机械购置与应用补贴额一览表（2026年）"]
["序号","大类","小类","品目","档次名称","基本配置和参数","最高补贴额（元）","备注"]
[{"$f":"ROW()-2","v":1},"种子初加工机械","种子初加工机械","种子清选机","生产率1.5—3t/h种子清选机","1.5t/h≤纯工作小时生产率＜3t/h",1000]
[{"$f":"ROW()-2","v":2},"种子初加工机械","种子初加工机械","种子清选机","生产率3—5t/h种子清选机","3t/h≤纯工作小时生产率＜5t/h",1800]
[3,"种子初加工机械","种子初加工机械","种子清选机","生产率5—15t/h种子清选机","5t/h≤纯工作小时生产率＜15t/h",3400]
[4,"种子初加工机械","种子初加工机械","种子清选机","生产率15—25t/h种子清选机","15t/h≤纯工作小时生产率＜25t/h",5000]
[5,"种子初加工机械","种子初加工机械","种子清选机","生产率25t/h及以上种子清选机","纯工作小时生产率≥25t/h",7000]
[6,"种子初加工机械","种子初加工机械","种子包衣机","5—10t种子包衣机","5t/h≤生产率＜10t/h",1500]
[7,"种子初加工机械","种子初加工机械","种子包衣机","10t及以上种子包衣机","生产率≥10t/h",2500]
[8,"种植业废弃物处理设备","农田废弃物收集设备","残膜回收机","工作幅宽1—2m残膜回收机","1m≤工作幅宽＜2m",400]
[9,"种植业废弃物处理设备","农田废弃物收集设备","残膜回收机","工作幅宽2—3m残膜回收机","2m≤工作幅宽＜3m",600]
[10,"种植业废弃物处理设备","农田废弃物收集设备","残膜回收机","工作幅宽>3m残膜回收机","工作幅宽>3m",800]
[11,"种植业废弃物处理设备","农田废弃物收集设备","残膜回收机","工作幅宽1—2m集膜箱残膜回收机","1m≤工作幅宽＜2m；集膜箱总容积≥1m³；生产率≥1hm²/h",4000]
[12,"种植业废弃物处理设备","农田废弃物收集设备","残膜回收机","工作幅宽2—3m集膜箱残膜回收机","2m≤工作幅宽＜3m；集膜箱总容积≥1m³；生产率≥1hm²/h",5000]
[13,"种植业废弃物处理设备","农田废弃物收集设备","残膜回收机","工作幅宽3以上集膜箱残膜回收机","工作幅宽≥3m；集膜箱总容积≥1m³；生产率≥1hm²/h",6000]
[14,"种植业废弃物处理设备","农作物废弃物处理设备","生物质气化设备","50—100kW沼气发电机组","50kW≤额定功率＜100kW；气缸数≥4",22000]
[15,"种植业废弃物处理设备","农作物废弃物处理设备","生物质气化设备","100—150kW沼气发电机组","100kW≤额定功率＜150kW；气缸数≥6",30000]
[16,"种植业废弃物处理设备","农作物废弃物处理设备","生物质气化设备","150—200kW沼气发电机组","150kW≤额定功率＜200kW；气缸数≥8",38000]
[17,"种植业废弃物处理设备","农作物废弃物处理设备","生物质气化设备","200kW及以上沼气发电机组","额定功率≥200kW；气缸数≥12",46000]
[18,"种植业废弃物处理设备","农作物废弃物处理设备","秸秆压块（粒、棒）机","0.2—0.5t/h秸秆压块（粒、棒）机","0.2t/h≤生产率＜0.5t/h；电机功率≥10kW",1300]
[19,"种植业废弃物处理设备","农作物废弃物处理设备","秸秆压块（粒、棒）机","0.5—1.5t/h秸秆压块（粒、棒）机","0.5t/h≤生产率＜1.5t/h；电机功率≥50kW",2600]
[20,"种植业废弃物处理设备","农作物废弃物处理设备","秸秆压块（粒、棒）机","1.5t/h及以上秸秆压块（粒、棒）机","生产率≥1.5t/h；电机功率≥75kW",4000]
[21,"种植业废弃物处理设备","农作物废弃物处理设备","秸秆压块（粒、棒）机","平模压块机","平模直径≥200mm；电机功率≥15kW",800]
[22,"种植业废弃物处理设备","农作物废弃物处理设备","秸秆压块（粒、棒）机","环模直径200—250mm压块机","200mm≤环模直径＜250mm；5kW≤电机功率＜17kW",2500]
[23,"种植业废弃物处理设备","农作物废弃物处理设备","秸秆压块（粒、棒）机","环模直径250mm及以上压块机","环模直径≥250mm；电机功率≥17kW",3500]
[24,"种植施肥机械","种子播前处理和育苗机械设备","种子催芽机","生产率20kg/h及以上箱体式自动温控水稻种子催芽机","箱体式；自动温控喷淋装置；催芽生产率≥20kg/h",500]
[25,"种植施肥机械","种子播前处理和育苗机械设备","育秧（苗）播种设备","生产率500盘/小时及以上秧盘播种成套设备","生产率≥500盘/小时；含铺底土、播种、洒水、覆土功能",3500]
[26,"种植施肥机械","耕整地播种作业机械（可含施肥功能）","铺膜（带）播种机","2—3行铺膜(带)播种机","播种行数2、3行，带覆膜功能",700]
[27,"种植施肥机械","耕整地播种作业机械（可含施肥功能）","铺膜（带）播种机","4—5行铺膜(带)播种机","播种行数4、5行，带覆膜功能",1400]
[28,"种植施肥机械","耕整地播种作业机械（可含施肥功能）","铺膜（带）播种机","6行以上铺膜(带)播种机","播种行数6行及以上，带覆膜功能",1800]
[29,"种植施肥机械","耕整地播种作业机械（可含施肥功能）","秸秆还田整地播种机","4行及以上秸秆还田整地播种机","与拖拉机配套的秸秆还田整地播种机；播种行数≥4行",2000]
[30,"种植施肥机械","栽植机械","抛秧机","乘坐式水稻抛秧机","结构型式：四轮乘坐式；抛秧方式：有序；发动机额定功率（或标定功率）≥13.5kW；工作行数≥7行",19000]
[31,"种植施肥机械","栽植机械","移栽机","1行秧苗移栽机","种植行数：1行",800]
[32,"种植施肥机械","栽植机械","移栽机","2行自走式秧苗移栽机","种植行数：2行；自走式",1200]
[33,"种植施肥机械","栽植机械","移栽机","4行及以上自走式秧苗移栽机","种植行数：4行及以上；自走式",2000]
[34,"种植施肥机械","栽植机械","移栽机","2—4行牵引式秧苗移栽机","种植行数：2、3行；牵引式",800]
[35,"种植施肥机械","栽植机械","移栽机","4行及以上牵引式秧苗移栽机","种植行数：4行及以上；牵引式",1200]
[36,"种植施肥机械","栽植机械","移栽机","2—4行四轮乘坐自走式秧苗移栽机","种植行数：2行；四轮乘坐自走式",5000]
[37,"种植施肥机械","栽植机械","移栽机","4行及以上四轮乘坐自走式秧苗移栽机","种植行数：4行及以上；四轮乘坐自走式",8000]
[38,"种植施肥机械","栽植机械","移栽机","2行手扶式全自动钵苗油菜移栽机","结构型式：手扶式；工作行数：2行；投苗方式：钵苗自动投苗；栽植器型式：挠性圆盘式；栽植频率：≥100株（穴）/（分·行）；栽植密度：≥6000株（穴）/亩；栽植深度可调，株距可调",20000]
[39,"种植施肥机械","栽植机械","移栽机","乘坐自走式打塘移栽浇水施肥复合机","结构形式：胶轮自走式或履带自走式；移栽行数1行；取苗形式：人工取苗；1000株/小时≤作业效率≤1500株/小时移栽器型式：钳夹式；含打塘装置、移栽装置、浇水装置、施肥装置",18000]
[40,"种植施肥机械","栽植机械","移栽机","牵引式打塘移栽浇水施肥复合机","结构形式：牵引式；移栽行数2行。移栽器型式：钳夹式；含打塘装置、移栽装置、浇水装置、施肥装置",15000]
[41,"种植施肥机械","施肥机械","施肥机","2行及以上施肥机","行数≥2行；肥箱容积≥1m³；结构形式：悬挂式、牵引式",500]
[42,"种植施肥机械","播种机械（可含施肥功能）","根（块）茎种子播种机","1行整秆式甘蔗种植机","结构型式:悬挂式；种植行数:1行",4000]
[43,"种植施肥机械","播种机械（可含施肥功能）","根（块）茎种子播种机","2行及以上整秆式甘蔗种植机","结构型式：悬挂式；种植行数≥2行",7000]
[44,"种植施肥机械","播种机械（可含施肥功能）","根（块）茎种子播种机","2行及以上段种式甘蔗种植机","结构型式：悬挂式；种植行数≥2行",3000]
[45,"田间监测及作业监控设备","田间作业监控设备","辅助驾驶（系统）设备（限用单北斗终端及单北斗辅助驾驶系统，含渔船用）","辅助驾驶（系统）设备","卫星接收机板卡类型及频点：北斗唯一；直线度精度≤2.5cm",1900,"需完成安装调试，能正常投入使用，作业面积达100亩及以上，才能办理购置补贴。"]
[46,"田间监测及作业监控设备","田间作业监控设备","田间作业监测终端","田间作业监测终端","卫星接收机板卡类型及频点：北斗信号；直线精度≤2.5cm",800,"需完成安装调试，确保设备能正常投入使用，才能办理补贴。"]
[47,"田间管理机械","中耕机械","中耕机","2行及以上悬挂式中耕机","悬挂式；作业行数≥2行；作业幅宽≥1.4m；施肥装置",1400]
[48,"田间管理机械","植保机械","农用（植保）无人驾驶航空器（可含撒播等功能）","10—20L多旋翼植保无人驾驶航空器","10L≤药液箱额定容量＜20L；多旋翼；电动、油动、油电混动；电动须配置智能电池系统，含智能电池2组及以上；具有避障系统；具有RTK的高精度卫星导航定位系统；具有电子围栏",4900,"1.多旋翼植保无人驾驶航空器是由两个以上旋翼（含两个）组成，并通过多个旋翼在空气中旋转产生升力和拉力实现飞行并进行施药作业的无人飞机。2.智能电池系统由智能电池和智能电池充电器组成，具备过充保护、过放保护、短路保护和充放电使用次数显示等功能。\n3.避障系统是指通过雷达或多目视觉等传感器主动检测障碍物并能实时规避的系统，通常有前避障、前后避障或绕障，不含使用航线规划绕障。"]
[49,"田间管理机械","植保机械","农用（植保）无人驾驶航空器（可含撒播等功能）","20—30L多旋翼植保无人驾驶航空器","20L≤药液箱额定容量＜30L；多旋翼；电动、油动、油电混动；电动须配置智能电池系统，含智能电池2组及以上；具有避障系统；具有RTK的高精度卫星导航定位系统；具有电子围栏",7300]
[50,"田间管理机械","植保机械","农用（植保）无人驾驶航空器（可含撒播等功能）","30—50L多旋翼植保无人驾驶航空器","30L≤药液箱额定容量＜50L；多旋翼；电动、油动、油电混动；电动须配置智能电池系统，含智能电池2组及以上；具有避障系统；具有RTK的高精度卫星导航定位系统；具有电子围栏",9800]
[51,"田间管理机械","植保机械","农用（植保）无人驾驶航空器（可含撒播等功能）","50L及以上多旋翼植保无人驾驶航空器","药液箱额定容量≥50L；多旋翼；电动、油动、油电混动；电动须配置智能电池系统，含智能电池2组及以上；具有避障系统；具有RTK的高精度卫星导航定位系统；具有电子围栏",11800]
[52,"田间管理机械","植保机械","农用（植保）无人驾驶航空器（可含撒播等功能）","15—25L单旋翼植保无人驾驶航空器","15L≤药液箱额定容量＜25L；单旋翼；电动、油动、油电混动；电动须配置智能电池系统，含智能电池2组及以上；具有避障系统；具有RTK的高精度卫星导航定位系统；具有电子围栏",7300]
[53,"田间管理机械","植保机械","农用（植保）无人驾驶航空器（可含撒播等功能）","25L及以上单旋翼植保无人驾驶航空器","药液箱额定容量≥25L；单旋翼；电动、油动、油电混动；电动须配置智能电池系统，含智能电池2组及以上；具有避障系统；具有RTK的高精度卫星导航定位系统；具有电子围栏",9800]
[54,"田间管理机械","修剪防护管理机械","农用升降作业平台","自走式果园作业平台","结构型式：自走式；驱动方式：两轮驱动、四轮驱动、履带式；升降机构类型：液压式；举升负载量≥250kg；最小离地间隙≥110mm；配套动力：电动机≥1.45kW、汽油机、柴油机≥5kW",4000]
[55,"田间管理机械","修剪防护管理机械","枝条切碎机","刀辊（盘）直径50-300mm枝条切碎机","50mm≤辊（盘）直径＜300mm；刀片（锤片）数量≥2个；结构型式：盘式、鼓式；配套动力：汽油机、柴油机、电机≥4.7kW或拖拉机；切削直径≥50mm",550]
[56,"田间管理机械","修剪防护管理机械","枝条切碎机","刀辊（盘）直径300mm及以上枝条切碎机","辊（盘）直径≥300mm；刀片（锤片）数量≥2个；结构型式：盘式、鼓式；配套动力：汽油机、柴油机、电机≥7.35kW或拖拉机；切削直径≥75mm",740]
[57,"天然橡胶初加工机械","天然橡胶初加工机械","生胶成型设备","天然橡胶初加工专用绉片机","电动机；绉片装置；功率≥11kW",12000]
[58,"天然橡胶初加工机械","天然橡胶初加工机械","生胶成型设备","天然橡胶初加工专用锤磨机","电动机；锤磨装置；功率≥30kW",20000]
[59,"天然橡胶初加工机械","天然橡胶初加工机械","生胶打包机","天然橡胶初加工专用打包机","电动机；打包装置；功率≥7.5kW",21000]
[60,"饲料（草）收获加工运输设备","饲料（草）收获机械","割草（压扁）机","1.1—1.8m往复式割草机","1.1m≤割幅宽度＜1.8m；往复式",620]
[61,"饲料（草）收获加工运输设备","饲料（草）收获机械","割草（压扁）机","1.8m及以上往复式割草机","割幅宽度≥1.8m；往复式",1600]
[62,"饲料（草）收获加工运输设备","饲料（草）收获机械","割草（压扁）机","0.8—1.3m旋转式割草机","0.8m≤割幅宽度＜1.3m；旋转式",550]
[63,"饲料（草）收获加工运输设备","饲料（草）收获机械","割草（压扁）机","1.3m及以上旋转式割草机","割幅宽度≥1.3m；旋转式",1800]
[64,"饲料（草）收获加工运输设备","饲料（草）收获机械","草捆包膜机","50cm≤包膜圆草捆直径＜100cm圆草捆包膜机","单一包膜作业；50cm≤包膜圆草捆直径＜100cm",900]
[65,"饲料（草）收获加工运输设备","饲料（草）收获机械","草捆包膜机","包膜圆草捆直径≥100cm圆草捆包膜机","单一包膜作业；包膜圆草捆直径≥100cm",2000]
[{"$f":"ROW()-2","v":66},"饲料（草）收获加工运输设备","饲料（草）收获机械","打捆包膜机","草捆直径500—900mm圆草捆打捆包膜一体机","挂接方式：固定式；500mm≤适用草捆直径范围＜900mm",4000]
[67,"饲料（草）收获加工运输设备","饲料（草）收获机械","打捆包膜机","草捆直径900mm及以上圆草捆打捆包膜一体机","挂接方式：固定式或牵引式；适用草捆直径范围≥900mm",6000]
[68,"饲料（草）收获加工运输设备","饲料（草）加工机械","颗粒饲料压制机","平模颗粒饲料压制机","平模直径≥200mm；电机功率≥15kW",800]
[69,"饲料（草）收获加工运输设备","饲料（草）加工机械","颗粒饲料压制机","环模直径200—250mm颗粒饲料压制机","200mm≤环模直径＜250mm；5kW≤电机功率＜17kW",2500]
[70,"饲料（草）收获加工运输设备","饲料（草）加工机械","颗粒饲料压制机","环模直径250mm及以上颗粒饲料压制机","环模直径≥250mm；电机功率≥17kW",3500]
[71,"饲料（草）收获加工运输设备","饲料（草）加工机械","饲料膨化机","单螺杆秸秆膨化机","螺杆数量1个；主机配套动力≥30kW；螺杆最大直径≥150mm",2000]
[72,"饲料（草）收获加工运输设备","饲料（草）加工机械","饲料膨化机","双螺杆秸秆膨化机","螺杆数量2个；主机配套动力≥30kW；螺杆最大直径≥120mm",3000]
[73,"饲料（草）收获加工运输设备","饲料（草）搬运机械","饲草捆收集机","功率≥20kW及以上自走式饲草捆收集机","型式：自走式；发动机标定功率≥20kW",5000]
[74,"饲料（草）收获加工运输设备","饲料（草）搬运机械","饲草捆收集机","牵引式饲草捆收集机","型式：牵引式；配套牵引动力范围≥58kW",3000]
[75,"水产养殖机械","水质调控设备","水质调控监控设备","水产养殖水质智能监控设备(具有测量水温、溶氧、PH值等功能)","数据传输方式为4G及以上；监控通道数≥4个；具有水温、溶氧、酸碱度PH值等测量功能",900,"需完成安装调试，确保设备能正常投入使用，才能办理补贴。"]
[76,"收获机械","糖料作物收获机械","甘蔗割铺（集条、集堆）机","悬挂式甘蔗割铺机","结构型式：悬挂式 ，纯工作小时生产率≥0.1hm²/h",1800]
[77,"收获机械","糖料作物收获机械","甘蔗割铺（集条、集堆）机","50kW及以上自走式甘蔗割堆机","结构型式：自走式，功率≥50kW，纯工作小时生产率≥0.12hm2/h或10t/h，具有集（卸）蔗装置，额定堆放量（额定收集质量）≥200kg，具有普通驾驶室。",7200]
[78,"收获机械","糖料作物收获机械","甘蔗联合收获机","90kW以上整杆式甘蔗联合收割机","整杆式;功率≥90kW;额定喂入量≥3kg/s",100000]
[79,"收获机械","糖料作物收获机械","甘蔗联合收获机","90kW及以上切段式甘蔗联合收割机","切段式；功率≥90kW；最小额定喂入量≥2.5kg/s",153000]
[80,"收获机械","果菜茶烟草药收获机械","根（茎）类收获机","0.6—1m中药材挖掘机","0.6m≤作业幅宽≤1m；挖掘深度≥25cm",2000]
[81,"收获机械","果菜茶烟草药收获机械","根（茎）类收获机","1—1.8m中药材挖掘机中药材挖掘机","1m≤作业幅宽＜1.8m；挖掘深度≥25cm",3500]
[82,"收获机械","果菜茶烟草药收获机械","根（茎）类收获机","1.8m及以上中药材挖掘机中药材挖掘机","作业幅宽≥1.8m；挖掘深度≥25cm",4000]
[83,"收获机械","收获割台","玉米收获专用割台","4行玉米收获专用割台","工作行数：4行",4500]
[84,"收获机械","收获割台","玉米收获专用割台","5行及以上玉米收获专用割台","工作行数≥5行",6000]
[85,"收获机械","天然橡胶收获机械","割胶刀","自动割胶设备","固定式，自动割胶；空机重量≤5kg；最大割线作业长度≥150mm，刀次割胶时间≤90秒/刀次；电池续航能力满足连续120刀次以上作业需求",147,"需完成安装调试，并完成30次及以上实际割胶作业，才能办理补贴。"]
[86,"收获机械","粮食作物收获机械","脱粒机","生产率0.3t/h及以上脱粒机","生产率≥0.3t/h；结构型式：半喂入；非机械夹持式；主滚筒工作长度≥70cm；配套动力功率≥1kW",200]
[87,"收获机械","粮食作物收获机械","脱粒机","生产率3-5t/h玉米脱粒机","3t/h≤生产率＜5t/h；结构型式：玉米脱粒机；单滚筒或双滚筒；主滚筒工作长度≥70cm；配套动力功率：电机≥1.5kW，柴油机或汽油机或其它≥4kW",120]
[88,"收获机械","粮食作物收获机械","脱粒机","生产率5t/h及以上玉米脱粒机","生产率≥5t/h；结构型式：玉米脱粒机；双滚筒或多滚筒；主滚筒工作长度≥70cm；配套动力功率：电机≥2.2kW，柴油机或汽油机或其它≥4kW",180]
[89,"设施种植机械","食用菌生产设备","菌料灭菌设备","容积30—50m³蒸汽灭菌设备","蒸汽灭菌；30m³≤容积≤50m³；设计压力≥170kPa",12000]
[90,"设施种植机械","食用菌生产设备","菌料灭菌设备","容积50m³以上蒸汽灭菌设备","蒸汽灭菌；容积>50m³；设计压力≥170kPa",20000]
[91,"设施种植机械","食用菌生产设备","菌料装瓶（袋）机","手动供瓶（套袋）的食用菌料装瓶（袋）机","手动套袋（供瓶）",400]
[92,"设施种植机械","食用菌生产设备","菌料装瓶（袋）机","生产率700袋/小时及以上自动装袋机","自动套袋（供瓶）；生产率≥700袋/小时",3500]
[93,"设施种植机械","食用菌生产设备","菌料装瓶（袋）机","生产率600袋/小时及以上自动装袋扎口一体机","自动套袋（供瓶）、扎口；生产率≥600袋/小时",5000]
[94,"农用动力机械","拖拉机","手扶拖拉机","8马力及以上皮带传动手扶拖拉机","传动方式：皮带传动；功率≥8马力",660]
[95,"农用动力机械","拖拉机","手扶拖拉机","11马力及以上直联传动手扶拖拉机","传动方式：直联传动；功率≥11马力",1000]
[96,"农田基本建设机械","清理机械","捡（清）石机","捡石机","工作幅宽≥1.2m，作业深度≥10cm",2000]
[97,"粮油糖初加工机械","粮食初加工机械","粮食清选机","生产率3-10t/h风筛清选机","结构型式:风筛式；3t/h ≤纯工作小时生产率＜10t/h",700]
[98,"粮油糖初加工机械","粮食初加工机械","粮食清选机","生产率10-25t/h风筛清选机","结构型式:风筛式；10t/h≤纯工作小时生产率＜25t/h",900]
[99,"粮油糖初加工机械","粮食初加工机械","粮食清选机","生产率25t/h以上风筛清选机","结构型式:风筛式；纯工作小时生产率≥25t/h",1200]
[100,"粮油糖初加工机械","粮食初加工机械","粮食清选机","生产率3-10t/h复式清选机","结构型式:复式；3t/h≤纯工作小时生产率＜10t/h",900]
[101,"粮油糖初加工机械","粮食初加工机械","粮食清选机","生产率10-25t/h复式清选机","结构型式:复式；10t/h≤纯工作小时生产率＜25t/h",1100]
[102,"粮油糖初加工机械","粮食初加工机械","粮食清选机","生产率25t/h以上复式清选机","结构型式:复式；纯工作小时生产率≥25t/h",1500]
[103,"粮油糖初加工机械","粮食初加工机械","磨粉机","磨辊长度30-40cm磨粉机","30cm≤磨辊长度＜40cm；磨辊直径≥22cm；磨辊数量≥2个",2000]
[104,"粮油糖初加工机械","粮食初加工机械","磨粉机","磨辊长度40-50cm磨粉机","40cm≤磨辊长度＜50cm；磨辊直径≥22cm；磨辊数量≥2个",2500]
[105,"粮油糖初加工机械","粮食初加工机械","磨粉机","磨辊长度在50cm及以上磨粉机","磨辊长度≥50cm；磨辊直径≥22cm；磨辊数量≥2个",3000]
[106,"粮油糖初加工机械","油料初加工机械","油菜籽干燥机","批处理量2—4t循环式油菜籽烘干机","2t≤批处理量＜4t；循环式",6400]
[107,"粮油糖初加工机械","油料初加工机械","油菜籽干燥机","批处理量4—10t循环式油菜籽烘干机","4t≤批处理量＜10t；循环式",15900]
[108,"粮油糖初加工机械","油料初加工机械","油菜籽干燥机","批处理量10—20t循环式油菜籽烘干机","10t≤批处理量＜20t；循环式",22600]
[109,"粮油糖初加工机械","油料初加工机械","油菜籽干燥机","批处理量20—30t循环式油菜籽烘干机","20t≤批处理量＜30t；循环式",29000]
[110,"粮油糖初加工机械","油料初加工机械","油菜籽干燥机","批处理量30t及以上循环式油菜籽烘干机","批处理量≥30t；循环式",46900]
[111,"粮油糖初加工机械","油料初加工机械","油料果（籽）脱（剥）壳机","1—1.5t/h花生脱壳机","1t/h≤生产率＜1.5t/h",600]
[112,"粮油糖初加工机械","油料初加工机械","油料果（籽）脱（剥）壳机","1.5—3t/h花生脱壳机","1.5t/h≤生产率＜3t/h；含自动上料设备",2200]
[113,"粮油糖初加工机械","油料初加工机械","油料果（籽）脱（剥）壳机","3t/h及以上花生脱壳机","生产率≥3t/h；含自动上料、去杂设备",4200]
[114,"粮油糖初加工机械","油料初加工机械","油料果（籽）脱（剥）壳机","油茶果分级剥壳一体机","生产率（鲜果）≥1000kg/h，分级装置级数≥2，配备皮带传送提升装置、分级装置、剥壳装置、分离装置",21600]
[115,"粮油糖初加工机械","油料初加工机械","其他油料初加工机械","纯工作小时生产率10-50kg/h水代法取油机","结构型式：卧式或立式；电机总功率≥10kW；搅拌轴工作段长度≥350mm；10kg/h≤纯工作小时生产率≤50kg/h",10000]
[116,"粮油糖初加工机械","油料初加工机械","其他油料初加工机械","纯工作小时生产率50kg/h以上水代法取油机","结构型式：卧式或立式；电机总功率≥30kW；搅拌轴工作段长度≥2100mm；纯工作小时生产率>50kg/h",40000]
[117,"粮油糖初加工机械","糖料初加工机械","甘蔗除杂设备","配套总功率≥50kW，生产率≥15t/h甘蔗除杂设备","上料、除杂联合作业；配套总功率≥50kW，生产率≥15t/h",50000]
[118,"果菜茶初加工机械","果蔬初加工机械","果蔬分级机","分选等级5个及以上机械式水果分级机","机械式；分选等级≥5个；生产率≥5t/h",2500]
[119,"果菜茶初加工机械","果蔬初加工机械","果蔬分级机","分选等级8个及以上电子式水果分级机","电子式；分选等级≥8个；生产率≥3t/h",5000]
[120,"果菜茶初加工机械","果蔬初加工机械","果蔬分级机","分选等级16个及以上电子式水果分级机","电子式；分选等级≥16个；生产率≥10t/h",7000]
[121,"果菜茶初加工机械","果蔬初加工机械","脱蓬（脯）机","剥皮滚筒长度600-1200mm青核桃剥皮机","600mm≤剥皮滚筒长度＜1200mm；生产率≥500kg/h；配套动力功率≥1.5kW",600]
[122,"果菜茶初加工机械","果蔬初加工机械","脱蓬（脯）机","剥皮滚筒长度1200mm及以上青核桃剥皮机","剥皮滚筒长度≥1200mm；生产率≥1000kg/h；配套动力功率≥2.2kW",900]
[123,"果菜茶初加工机械","果蔬初加工机械","脱蓬（脯）机","剥皮滚筒长度600-1200mm带喂料机构青核桃剥皮机","600mm≤剥皮滚筒长度＜1200mm；喂料输送长度≥1500mm；生产率≥500kg/h；配套动力功率≥3kW",1000]
[124,"果菜茶初加工机械","果蔬初加工机械","脱蓬（脯）机","剥皮滚筒长度1200mm及以上带喂料机构青核桃剥皮机","剥皮滚筒长度≥1200mm；喂料输送长度≥1500mm；生产率≥1000kg/h；配套动力功率≥3.5kW",1300]
[125,"果菜茶初加工机械","果蔬初加工机械","脱蓬（脯）机","生产率300-1000kg/h青核桃剥皮自动化设备","非滚筒式，300kg/h≤生产率＜1000kg/h；含电机、自动喂料、自动卸料",600]
[126,"果菜茶初加工机械","果蔬初加工机械","脱蓬（脯）机","生产率1000-2000kg/h青核桃剥皮自动化设备","非滚筒式，1000kg/h≤生产率＜2000kg/h；含电机、自动喂料、自动卸料",1300]
[127,"果菜茶初加工机械","果蔬初加工机械","脱蓬（脯）机","生产率2000kg/h以上青核桃剥皮自动化设备","非滚筒式，生产率≥2000kg/h；含电机、自动喂料、自动卸料",1800]
[128,"果菜茶初加工机械","果蔬初加工机械","青果（豆）脱壳机","生产率300—1000kg/h澳洲坚果青皮脱皮机","600mm≤剥皮辊筒长度＜1000mm；300kg/h≤生产率＜1000kg/h，配套动力功率≥0.75kW",600]
[129,"果菜茶初加工机械","果蔬初加工机械","青果（豆）脱壳机","生产率1000—5000kg/h澳洲坚果青皮脱皮机","剥皮辊筒长度≥1000mm;剥皮辊筒数量≥4个；1000kg/h≤生产率＜5000kg/h，配套动力总功率≥3kW",1200]
[{"$f":"ROW()-2","v":130},"果菜茶初加工机械","果蔬初加工机械","青果（豆）脱壳机","生产率5000kg/h及以上澳洲坚果青皮脱皮机","剥皮辊筒长度≥1000mm;剥皮辊筒数量≥16个；生产率≥5000kg/h，配套动力总功率≥12kW",3000]
[131,"果菜茶初加工机械","果蔬初加工机械","果蔬去籽（核）机","生产率100－500kg/h简式花椒脱籽筛选机","脱籽滚筒工作长度≥270mm，清选筛型式：网孔振动筛；筛片层数≥4层；筛片面积≥0.5m2；100kg/h≤生产率＜500kg/h，配套动力总功率≥3kW",1500]
[132,"果菜茶初加工机械","果蔬初加工机械","果蔬去籽（核）机","生产率500kg/h及以上简式花椒脱籽筛选机","脱籽滚筒工作长度≥370mm，清选筛型式：网孔振动筛；筛片层数≥4层；筛片面积≥0.9m2；生产率≥500kg/h，配套动力总功率≥3kW",2800]
[133,"果菜茶初加工机械","茶叶初加工机械","茶叶做青机","茶叶综合做青机","滚筒容积≥2m³，滚筒内径≥110cm",1000]
[134,"果菜茶初加工机械","茶叶初加工机械","茶叶做青机","有效摊叶面积20m²以下茶叶摊青机、萎凋机、摊青萎凋机","有效摊叶面积＜20m²",1200]
[135,"果菜茶初加工机械","茶叶初加工机械","茶叶做青机","有效摊叶面积20m²及以上茶叶摊青机、萎凋机、摊青萎凋机","有效摊叶面积≥20m²",3000]
[136,"果菜茶初加工机械","茶叶初加工机械","茶叶杀青机","滚筒直径30-40cm、滚筒内部直段长度小于2000mm杀青机","结构型式：滚筒式；30cm≤滚筒直径＜40cm，滚筒内部直段长度＜2000mm",600]
[137,"果菜茶初加工机械","茶叶初加工机械","茶叶杀青机","滚筒直径30-40cm、滚筒内部直段长度大于等于2000mm杀青机","结构型式：滚筒式；30cm≤滚筒直径＜40cm；滚筒内部直段长度≥2000mm",1000]
[138,"果菜茶初加工机械","茶叶初加工机械","茶叶杀青机","滚筒直径40-60cm、滚筒内部直段长度小于2000mm杀青机","结构型式：滚筒式；30cm≤滚筒直径＜40cm，滚筒内部直段长度＜2000mm",700]
[139,"果菜茶初加工机械","茶叶初加工机械","茶叶杀青机","滚筒直径40-60cm、滚筒内部直段长度大于等于2000mm杀青机","结构型式：滚筒式；40cm≤滚筒直径＜60cm；滚筒内部直段长度≥2000mm",1300]
[140,"果菜茶初加工机械","茶叶初加工机械","茶叶杀青机","滚筒直径大于60cm及以上、滚筒内部直段长度小于2000mm杀青机","结构型式：滚筒式；滚筒直径≥60cm；滚筒内部直段长度＜2000mm",800]
[141,"果菜茶初加工机械","茶叶初加工机械","茶叶杀青机","滚筒直径60cm及以上、滚筒内部直段长度大于等于2000mm杀青机","结构型式：滚筒式；滚筒直径≥60cm；滚筒内部直段长度≥2000mm",1700]
[142,"果菜茶初加工机械","茶叶初加工机械","茶叶揉捻机","揉筒直径25-35cm揉捻机","25cm≤揉筒直径＜35cm；含动力",480]
[143,"果菜茶初加工机械","茶叶初加工机械","茶叶揉捻机","揉筒直径35-50cm揉捻机","35cm≤揉筒直径＜50cm；含动力",880]
[144,"果菜茶初加工机械","茶叶初加工机械","茶叶揉捻机","揉筒直径50-60cm揉捻机","50cm≤揉筒直径＜60cm；含动力",1400]
[145,"果菜茶初加工机械","茶叶初加工机械","茶叶揉捻机","揉筒直径60cm及以上揉捻机（含揉捻机组）","揉筒直径≥60cm；含动力",1800]
[146,"灌溉机械","喷灌机械","喷灌机","轻小型机组式喷灌机","移动方式：手抬式或手推式；2.5kW≤功率≤22kW",400]
[147,"灌溉机械","喷灌机械","喷灌机","管径50—65mm绞盘式/卷盘式喷灌机","配水软管材质：PE管；软管壁厚≥4.6mm；软管长度≥150m；50mm≤软管外径＜65mm",3500]
[148,"灌溉机械","喷灌机械","喷灌机","管径65—75mm绞盘式/卷盘式喷灌机","配水软管材质：PE管；软管壁厚≥5.8mm；软管长度≥200m；65mm≤软管外径＜75mm",4000]
[149,"灌溉机械","喷灌机械","喷灌机","管径75—85mm绞盘式/卷盘式喷灌机","配水软管材质：PE管；软管壁厚≥6mm；软管长度≥300m；75mm≤软管外径＜85mm",4500]
[150,"灌溉机械","喷灌机械","喷灌机","管径85mm及以上绞盘式/卷盘式喷灌机","配水软管材质：PE管；软管壁厚≥7.8mm；软管长度≥300m；软管外径≥85mm",5000]
[151,"灌溉机械","喷灌机械","喷灌机","大型喷灌机","中心支轴式喷灌机或者平移式喷灌机；跨距≥50m；桁架输水管外径≥159mm；喷头间距≤2.88m；塔架驱动部分电动机功率≥0.55千瓦/跨；塔架轮胎数量2—4个/跨",5000]
[152,"灌溉机械","微灌设备","微喷灌设备","流量10—50m³/h微喷灌系统（设备）","10m³/h≤流量＜50m³/h；出水口内径≥50mm；首部（按GB50485规定配备；含加压设备、过滤器、施肥（药）装置；量测和控制设备）",240]
[153,"灌溉机械","微灌设备","微喷灌设备","流量50m³/h及以上微喷灌系统（设备）","流量≥50m³/h；出水口内径≥50mm；首部（按GB50485规定配备；含加压设备、过滤器、施肥（药）装置；量测和控制设备）",350]
[154,"耕整地机械","耕地机械","其他耕地机械","单行悬挂式耕整打塘机","悬挂式；1.4m≤旋耕工作幅宽≤1.6m；起垄行数1行；打塘铲数量1套；含旋耕装置、起垄装置、打塘装置",1800]
[155,"耕整地机械","耕地机械","其他耕地机械","双行悬挂式耕整打塘机","悬挂式；2.3m≤旋耕工作幅宽≤2.5m；起垄行数2行；打塘铲数量2套；含旋耕装置、起垄装置、打塘装置",3000]
[156,"耕整地机械","整地机械","起垄机","1—1.5m起垄机","1m≤工作幅宽＜1.5m；含旋耕装置",400]
[157,"耕整地机械","整地机械","起垄机","1.5—2m起垄机","1.5m≤工作幅宽＜2m；含旋耕装置",1000]
[158,"耕整地机械","整地机械","起垄机","2—2.5m起垄机","2m≤工作幅宽＜2.5m；含旋耕装置",2000]
[159,"耕整地机械","整地机械","起垄机","2.5m及以上起垄机","工作幅宽≥2.5m；含旋耕装置",2500]
[160,"畜禽养殖机械","饲养设备","喂（送）料机","三层行车式喂料机","行车式；喂料机层数：3层；料斗数量：6个；料斗行程距离≥50m；含电机、驱动装 置、控制装置",2000]
[161,"畜禽养殖机械","饲养设备","喂（送）料机","料箱容积60升及以上自动干湿料喂料机","自动控制；料箱容积≥60L",780]
[162,"畜禽养殖机械","饲养设备","喂（送）料机","100—200m塞盘链式送料机","塞盘链式；配套电机功率≥1.5kW；塞盘直径≥40mm；100m≤料管长度＜200m；含电机、料斗、驱动装置、控制装置",5600]
[163,"畜禽养殖机械","饲养设备","喂（送）料机","200m以上塞盘链式送料机","塞盘链式；配套电机功率≥1.5kW；塞盘直径≥40mm；料管长度≥200m；含电机、料斗、驱动装置、控制装置",6800]
[164,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","0.75kW及以上刮粪板式清粪机","刮板式；电机额定功率≥0.75kW；刮粪板数量≥1；工作幅宽（刮板宽度）≥1m",300]
[165,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","1.5kW及以上刮粪板式清粪机","刮板式；电机额定功率≥1.5kW；刮粪板数量≥2；工作幅宽（刮板宽度）≥1m",600]
[166,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","1.5kW及以上不锈钢刮粪板式清粪机","不锈钢刮板式；电机额定功率≥1.5kW；刮粪板数量≥2；工作幅宽（刮板宽度）≥1m",900]
[167,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","90m—200m²输送带式清粪机","输送带式；90m²≤输送带面积＜200m²",2000,"输送带面积=粪带宽度×辊筒上方粪带长度×粪带层数"]
[168,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","200—300m²输送带式清粪机","输送带式；200m²≤输送带面积＜300m²",3300]
[169,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","300—400m²输送带式清粪机","输送带式；300m²≤输送带面积＜400m²",4400]
[170,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","400—500m²输送带式清粪机","输送带式；400m²≤输送带面积＜500m²",5500]
[171,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","清粪机","500m²及以上输送带式清粪机","输送带式；输送带面积≥500m²",6600]
[172,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪污固液分离机","筛筒面积0.2m²—0.5m²粪污固液分离机","0.2m²≤筛筒面积＜0.5m²；结构型式：螺旋挤压式",1700,"筛筒面积=3.14×筛简直径×筛筒长度"]
[173,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪污固液分离机","筛筒面积0.5m²及以上粪污固液分离机","筛筒面积≥0.5m²；结构型式：螺旋挤压式",2200]
[174,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪污固液分离机","斜筛面积0.35m²—0.8m²粪污固液分离机","0.35m²≤斜筛面积≤0.8m²；结构型式：筛分（斜筛）+螺旋挤压式",3000]
[175,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪污固液分离机","斜筛面积0.8m²以上粪污固液分离机","斜筛面积＞0.8m²；结构型式：筛分（斜筛）+螺旋挤压式；配备振动电机",3600]
[176,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便发酵处理设备","5—10m³罐式畜禽粪便发酵处理机","罐式；5m³≤盛料容器容积＜10m³",16000]
[177,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便发酵处理设备","10—30m³罐式畜禽粪便发酵处理机","罐式；10m³≤盛料容器容积＜30m³",30000]
[178,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便发酵处理设备","30—50m³罐式畜禽粪便发酵处理机","罐式；30m³≤盛料容器容积＜50m³",60000]
[179,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便发酵处理设备","50—80m³罐式畜禽粪便发酵处理机","罐式；50m³≤盛料容器容积＜80m³",90000]
[180,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便发酵处理设备","80—100m³罐式畜禽粪便发酵处理机","罐式；80m³≤盛料容器容积＜100m³",100000]
[181,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便发酵处理设备","100m³及以上罐式畜禽粪便发酵处理机","罐式；盛料容器容积≥100m³",120000]
[182,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便发酵处理设备","10—30m³层叠式畜禽粪便发酵处理机","层叠式；10m³≤盛料容器容积＜30m³",21000]
[183,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便发酵处理设备","30—50m³层叠式畜禽粪便发酵处理机","层叠式；30m³≤盛料容器容积＜50m³",43000]
[184,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便发酵处理设备","50m³及以上层叠式畜禽粪便发酵处理机","层叠式；盛料容器容积≥50m³",50000]
[185,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便发酵处理设备","3—10m³其他式畜禽粪便发酵处理机","其他式；3m³≤盛料容器容积＜10m³",10000]
[186,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便发酵处理设备","10m³及以上其他式畜禽粪便发酵处理机","其他式；盛料容器容积≥10m³",18000]
[187,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便干燥设备","200kg≤一次进料＜500kg畜禽粪便干燥设备","加热形式不限，200kg≤一次进料＜500kg，抽湿风机功率≥37W，电加热烘干机加热功率需≥25kW，煤加热烘干机抽火功率需≥370kW",2000]
[188,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便干燥设备","500kg≤一次进料＜2000kg畜禽粪便干燥设备","加热形式不限，500kg≤一次进料＜2000kg抽湿风机功率≥370W，电加热烘干机加热功率需≥40kW，煤加热烘干机抽火功率需≥550kW",4000]
[189,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便干燥设备","2000kg≤一次进料＜5000kg畜禽粪便干燥设备","加热形式不限，2000kg≤一次进料＜5000kg，抽湿风机功率≥750W，电加热烘干机加热功率需≥80kW，煤加热烘干机抽火功率需≥1100kW",8000]
[190,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","1.5—3m电动有机废弃物好氧发酵翻堆机","1.5m≤工作幅宽＜3m；配套动力型式：电动机；配套总功率≥7kW",2100]
[191,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","3—4m电动有机废弃物好氧发酵翻堆机","3m≤工作幅宽＜4m；配套动力型式：电动机；配套总功率≥10kW",3100]
[192,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","4m及以上电动有机废弃物好氧发酵翻堆机","工作幅宽≥4m；配套动力型式：电动机；配套总功率≥12kW",4000]
[193,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","翻堆高度（深度）1.5m及以上电动有机废弃物好氧发酵翻堆机","工作幅宽≥0.9m；配套动力型式：电动机；配套总功率≥23kW；物料最大堆放高度（深度）≥1.5m",5000]
[{"$f":"ROW()-2","v":194},"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","2—2.5m油动有机废弃物好氧发酵翻堆机","2m≤工作幅宽＜2.5m；配套动力型式：柴油机；配套总功率≥22.1kW",8000]
[195,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","2.5—3m油动有机废弃物好氧发酵翻堆机","2.5m≤工作幅宽＜3m；配套动力型式：柴油机；配套总功率≥51.5kW",15000]
[196,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","畜禽粪便翻堆设备","3m及以上油动有机废弃物好氧发酵翻堆机","工作幅宽≥3m；配套动力型式：柴油机；配套总功率≥73.5kW",22000]
[197,"畜禽养殖废弃物及病死畜禽处理设备","畜禽粪污资源化利用设备","沼液沼渣抽排设备","非自走式沼液沼渣抽排设备","型式：非自走式；罐体容积≥3m³；抽排设备配套动力额定功率≥6.3kW",900]
[198,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","0.5—1m³降解式病死畜禽无害化处理","降解法；0.5m³≤箱体容积＜1m³",2000]
[199,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","1—2m³降解式病死畜禽无害化处理","降解法；1m³≤箱体容积＜2m³",4000]
[200,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","2—3m³降解式病死畜禽无害化处理设备","降解法；2m³≤箱体容积＜3m³",6000]
[201,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","3m³及以上降解式病死畜禽无害化处理设备","降解法；箱体容积≥3m³",12000]
[202,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","0.9—2m³干化式病死畜禽无害化处理设备","干化法；0.9m³≤箱体容积＜2m³；工作压力≥200kPa（属于压力容器）",18000]
[203,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","2—4m³干化式病死畜禽无害化处理设备","干化法；2m³≤箱体容积＜4m³；工作压力≥200kPa（属于压力容器）",31000]
[204,"畜禽养殖废弃物及病死畜禽处理设备","病死畜禽储运及处理设备","病死畜禽处理设备","4m³及以上干化式病死畜禽无害化处理设备","干化法；箱体容积≥4m³；工作压力≥200kPa（属于压力容器）",41000]

{"sheet":"204个档次","index":1,"n_rows":205,"n_cols":3,"rows_kept":205}
["列E","计数","占比"]
["0.2—0.5t/h秸秆压块（粒、棒）机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["0.5—1.5t/h秸秆压块（粒、棒）机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["0.5—1m³降解式病死畜禽无害化处理",1,{"v":0.0048780487804878,"d":"0.5%"}]
["0.6—1m中药材挖掘机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["0.75kW及以上刮粪板式清粪机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["0.8—1.3m旋转式割草机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["0.9—2m³干化式病死畜禽无害化处理设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1.1—1.8m往复式割草机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1.3m及以上旋转式割草机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1.5—2m起垄机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1.5—3m电动有机废弃物好氧发酵翻堆机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1.5—3t/h花生脱壳机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1.5kW及以上不锈钢刮粪板式清粪机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1.5kW及以上刮粪板式清粪机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1.5t/h及以上秸秆压块（粒、棒）机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1.8m及以上往复式割草机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1.8m及以上中药材挖掘机中药材挖掘机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["100—150kW沼气发电机组",1,{"v":0.0048780487804878,"d":"0.5%"}]
["100—200m塞盘链式送料机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["100m³及以上罐式畜禽粪便发酵处理机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["10—20L多旋翼植保无人驾驶航空器",1,{"v":0.0048780487804878,"d":"0.5%"}]
["10—30m³层叠式畜禽粪便发酵处理机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["10—30m³罐式畜禽粪便发酵处理机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["10m³及以上其他式畜禽粪便发酵处理机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["10t及以上种子包衣机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1—1.5m起垄机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1—1.5t/h花生脱壳机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1—1.8m中药材挖掘机中药材挖掘机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["11马力及以上直联传动手扶拖拉机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1—2m³降解式病死畜禽无害化处理",1,{"v":0.0048780487804878,"d":"0.5%"}]
["150—200kW沼气发电机组",1,{"v":0.0048780487804878,"d":"0.5%"}]
["15—25L单旋翼植保无人驾驶航空器",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1行秧苗移栽机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["1行整秆式甘蔗种植机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2.5—3m油动有机废弃物好氧发酵翻堆机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2.5m及以上起垄机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2000kg≤一次进料＜5000kg畜禽粪便干燥设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["200—300m²输送带式清粪机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["200kg≤一次进料＜500kg畜禽粪便干燥设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["200kW及以上沼气发电机组",1,{"v":0.0048780487804878,"d":"0.5%"}]
["200m以上塞盘链式送料机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["20—30L多旋翼植保无人驾驶航空器",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2—2.5m起垄机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2—2.5m油动有机废弃物好氧发酵翻堆机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2—3m³降解式病死畜禽无害化处理设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2—3行铺膜(带)播种机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2—4m³干化式病死畜禽无害化处理设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2—4行牵引式秧苗移栽机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2—4行四轮乘坐自走式秧苗移栽机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["25L及以上单旋翼植保无人驾驶航空器",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2行及以上段种式甘蔗种植机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2行及以上施肥机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2行及以上悬挂式中耕机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2行及以上整秆式甘蔗种植机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2行手扶式全自动钵苗油菜移栽机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["2行自走式秧苗移栽机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["300—400m²输送带式清粪机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["30—50L多旋翼植保无人驾驶航空器",1,{"v":0.0048780487804878,"d":"0.5%"}]
["30—50m³层叠式畜禽粪便发酵处理机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["30—50m³罐式畜禽粪便发酵处理机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["3—10m³其他式畜禽粪便发酵处理机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["3—4m电动有机废弃物好氧发酵翻堆机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["3m³及以上降解式病死畜禽无害化处理设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["3m及以上油动有机废弃物好氧发酵翻堆机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["3t/h及以上花生脱壳机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["400—500m²输送带式清粪机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["4—5行铺膜(带)播种机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["4m³及以上干化式病死畜禽无害化处理设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["4m及以上电动有机废弃物好氧发酵翻堆机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["4行及以上秸秆还田整地播种机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["4行及以上牵引式秧苗移栽机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["4行及以上四轮乘坐自走式秧苗移栽机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["4行及以上自走式秧苗移栽机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["4行玉米收获专用割台",1,{"v":0.0048780487804878,"d":"0.5%"}]
["500kg≤一次进料＜2000kg畜禽粪便干燥设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["500m²及以上输送带式清粪机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["50—100kW沼气发电机组",1,{"v":0.0048780487804878,"d":"0.5%"}]
["50—80m³罐式畜禽粪便发酵处理机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["50cm≤包膜圆草捆直径＜100cm圆草捆包膜机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["50kW及以上自走式甘蔗割堆机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["50L及以上多旋翼植保无人驾驶航空器",1,{"v":0.0048780487804878,"d":"0.5%"}]
["50m³及以上层叠式畜禽粪便发酵处理机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["5—10m³罐式畜禽粪便发酵处理机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["5—10t种子包衣机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["5行及以上玉米收获专用割台",1,{"v":0.0048780487804878,"d":"0.5%"}]
["6行以上铺膜(带)播种机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["80—100m³罐式畜禽粪便发酵处理机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["8马力及以上皮带传动手扶拖拉机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["90kW及以上切段式甘蔗联合收割机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["90kW以上整杆式甘蔗联合收割机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["90m—200m²输送带式清粪机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["包膜圆草捆直径≥100cm圆草捆包膜机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["剥皮滚筒长度1200mm及以上带喂料机构青核桃剥皮机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["剥皮滚筒长度1200mm及以上青核桃剥皮机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["剥皮滚筒长度600-1200mm带喂料机构青核桃剥皮机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["剥皮滚筒长度600-1200mm青核桃剥皮机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["草捆直径500—900mm圆草捆打捆包膜一体机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["草捆直径900mm及以上圆草捆打捆包膜一体机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["茶叶综合做青机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["乘坐式水稻抛秧机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["乘坐自走式打塘移栽浇水施肥复合机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["纯工作小时生产率10-50kg/h水代法取油机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["纯工作小时生产率50kg/h以上水代法取油机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["大型喷灌机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["单螺杆秸秆膨化机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["单行悬挂式耕整打塘机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["刀辊（盘）直径300mm及以上枝条切碎机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["刀辊（盘）直径50-300mm枝条切碎机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["翻堆高度（深度）1.5m及以上电动有机废弃物好氧发酵翻堆机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["非自走式沼液沼渣抽排设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["分选等级16个及以上电子式水果分级机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["分选等级5个及以上机械式水果分级机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["分选等级8个及以上电子式水果分级机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["辅助驾驶（系统）设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["工作幅宽>3m残膜回收机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["工作幅宽1—2m残膜回收机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["工作幅宽1—2m集膜箱残膜回收机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["工作幅宽2—3m残膜回收机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["工作幅宽2—3m集膜箱残膜回收机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["工作幅宽3以上集膜箱残膜回收机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["功率≥20kW及以上自走式饲草捆收集机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["管径50—65mm绞盘式/卷盘式喷灌机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["管径65—75mm绞盘式/卷盘式喷灌机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["管径75—85mm绞盘式/卷盘式喷灌机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["管径85mm及以上绞盘式/卷盘式喷灌机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["滚筒直径30-40cm、滚筒内部直段长度大于等于2000mm杀青机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["滚筒直径30-40cm、滚筒内部直段长度小于2000mm杀青机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["滚筒直径40-60cm、滚筒内部直段长度大于等于2000mm杀青机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["滚筒直径40-60cm、滚筒内部直段长度小于2000mm杀青机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["滚筒直径60cm及以上、滚筒内部直段长度大于等于2000mm杀青机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["滚筒直径大于60cm及以上、滚筒内部直段长度小于2000mm杀青机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["环模直径200—250mm颗粒饲料压制机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["环模直径200—250mm压块机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["环模直径250mm及以上颗粒饲料压制机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["环模直径250mm及以上压块机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["捡石机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["料箱容积60升及以上自动干湿料喂料机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["流量10—50m³/h微喷灌系统（设备）",1,{"v":0.0048780487804878,"d":"0.5%"}]
["流量50m³/h及以上微喷灌系统（设备）",1,{"v":0.0048780487804878,"d":"0.5%"}]
["磨辊长度30-40cm磨粉机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["磨辊长度40-50cm磨粉机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["磨辊长度在50cm及以上磨粉机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["配套总功率≥50kW，生产率≥15t/h甘蔗除杂设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["批处理量10—20t循环式油菜籽烘干机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["批处理量20—30t循环式油菜籽烘干机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["批处理量2—4t循环式油菜籽烘干机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["批处理量30t及以上循环式油菜籽烘干机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["批处理量4—10t循环式油菜籽烘干机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["平模颗粒饲料压制机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["平模压块机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["牵引式打塘移栽浇水施肥复合机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["牵引式饲草捆收集机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["轻小型机组式喷灌机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["容积30—50m³蒸汽灭菌设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["容积50m³以上蒸汽灭菌设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["揉筒直径25-35cm揉捻机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["揉筒直径35-50cm揉捻机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["揉筒直径50-60cm揉捻机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["揉筒直径60cm及以上揉捻机（含揉捻机组）",1,{"v":0.0048780487804878,"d":"0.5%"}]
["三层行车式喂料机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["筛筒面积0.2m²—0.5m²粪污固液分离机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["筛筒面积0.5m²及以上粪污固液分离机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率0.3t/h及以上脱粒机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率1.5—3t/h种子清选机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率1000-2000kg/h青核桃剥皮自动化设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率1000—5000kg/h澳洲坚果青皮脱皮机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率100－500kg/h简式花椒脱籽筛选机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率10-25t/h风筛清选机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率10-25t/h复式清选机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率15—25t/h种子清选机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率2000kg/h以上青核桃剥皮自动化设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率20kg/h及以上箱体式自动温控水稻种子催芽机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率25t/h及以上种子清选机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率25t/h以上风筛清选机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率25t/h以上复式清选机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率300—1000kg/h澳洲坚果青皮脱皮机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率300-1000kg/h青核桃剥皮自动化设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率3-10t/h风筛清选机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率3-10t/h复式清选机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率3-5t/h玉米脱粒机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率3—5t/h种子清选机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率5000kg/h及以上澳洲坚果青皮脱皮机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率500kg/h及以上简式花椒脱籽筛选机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率500盘/小时及以上秧盘播种成套设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率5—15t/h种子清选机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率5t/h及以上玉米脱粒机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率600袋/小时及以上自动装袋扎口一体机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生产率700袋/小时及以上自动装袋机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["手动供瓶（套袋）的食用菌料装瓶（袋）机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["双螺杆秸秆膨化机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["双行悬挂式耕整打塘机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["水产养殖水质智能监控设备(具有测量水温、溶氧、PH值等功能)",1,{"v":0.0048780487804878,"d":"0.5%"}]
["天然橡胶初加工专用锤磨机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["天然橡胶初加工专用打包机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["天然橡胶初加工专用绉片机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["田间作业监测终端",1,{"v":0.0048780487804878,"d":"0.5%"}]
["斜筛面积0.35m²—0.8m²粪污固液分离机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["斜筛面积0.8m²以上粪污固液分离机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["悬挂式甘蔗割铺机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["油茶果分级剥壳一体机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["有效摊叶面积20m²及以上茶叶摊青机、萎凋机、摊青萎凋机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["有效摊叶面积20m²以下茶叶摊青机、萎凋机、摊青萎凋机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["自动割胶设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["自走式果园作业平台",1,{"v":0.0048780487804878,"d":"0.5%"}]

{"sheet":"63个品目","index":2,"n_rows":64,"n_cols":3,"rows_kept":64}
["列D","计数","占比"]
["病死畜禽处理设备",7,{"v":0.0341463414634146,"d":"3.4%"}]
["残膜回收机",6,{"v":0.0292682926829268,"d":"2.9%"}]
["草捆包膜机",2,{"v":0.00975609756097561,"d":"1.0%"}]
["茶叶揉捻机",4,{"v":0.0195121951219512,"d":"2.0%"}]
["茶叶杀青机",6,{"v":0.0292682926829268,"d":"2.9%"}]
["茶叶做青机",3,{"v":0.0146341463414634,"d":"1.5%"}]
["畜禽粪便发酵处理设备",11,{"v":0.0536585365853659,"d":"5.4%"}]
["畜禽粪便翻堆设备",7,{"v":0.0341463414634146,"d":"3.4%"}]
["畜禽粪便干燥设备",3,{"v":0.0146341463414634,"d":"1.5%"}]
["畜禽粪污固液分离机",4,{"v":0.0195121951219512,"d":"2.0%"}]
["打捆包膜机",2,{"v":0.00975609756097561,"d":"1.0%"}]
["辅助驾驶（系统）设备（限用单北斗终端及单北斗辅助驾驶系统，含渔船用）",1,{"v":0.0048780487804878,"d":"0.5%"}]
["甘蔗除杂设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["甘蔗割铺（集条、集堆）机",2,{"v":0.00975609756097561,"d":"1.0%"}]
["甘蔗联合收获机",2,{"v":0.00975609756097561,"d":"1.0%"}]
["割草（压扁）机",4,{"v":0.0195121951219512,"d":"2.0%"}]
["割胶刀",1,{"v":0.0048780487804878,"d":"0.5%"}]
["根（茎）类收获机",3,{"v":0.0146341463414634,"d":"1.5%"}]
["根（块）茎种子播种机",3,{"v":0.0146341463414634,"d":"1.5%"}]
["果蔬分级机",3,{"v":0.0146341463414634,"d":"1.5%"}]
["果蔬去籽（核）机",2,{"v":0.00975609756097561,"d":"1.0%"}]
["捡（清）石机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["秸秆还田整地播种机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["秸秆压块（粒、棒）机",6,{"v":0.0292682926829268,"d":"2.9%"}]
["菌料灭菌设备",2,{"v":0.00975609756097561,"d":"1.0%"}]
["菌料装瓶（袋）机",3,{"v":0.0146341463414634,"d":"1.5%"}]
["颗粒饲料压制机",3,{"v":0.0146341463414634,"d":"1.5%"}]
["粮食清选机",6,{"v":0.0292682926829268,"d":"2.9%"}]
["磨粉机",3,{"v":0.0146341463414634,"d":"1.5%"}]
["农用（植保）无人驾驶航空器（可含撒播等功能）",6,{"v":0.0292682926829268,"d":"2.9%"}]
["农用升降作业平台",1,{"v":0.0048780487804878,"d":"0.5%"}]
["抛秧机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["喷灌机",6,{"v":0.0292682926829268,"d":"2.9%"}]
["铺膜（带）播种机",3,{"v":0.0146341463414634,"d":"1.5%"}]
["其他耕地机械",2,{"v":0.00975609756097561,"d":"1.0%"}]
["其他油料初加工机械",2,{"v":0.00975609756097561,"d":"1.0%"}]
["起垄机",4,{"v":0.0195121951219512,"d":"2.0%"}]
["青果（豆）脱壳机",3,{"v":0.0146341463414634,"d":"1.5%"}]
["清粪机",8,{"v":0.0390243902439024,"d":"3.9%"}]
["生胶成型设备",2,{"v":0.00975609756097561,"d":"1.0%"}]
["生胶打包机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["生物质气化设备",4,{"v":0.0195121951219512,"d":"2.0%"}]
["施肥机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["手扶拖拉机",2,{"v":0.00975609756097561,"d":"1.0%"}]
["水质调控监控设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["饲草捆收集机",2,{"v":0.00975609756097561,"d":"1.0%"}]
["饲料膨化机",2,{"v":0.00975609756097561,"d":"1.0%"}]
["田间作业监测终端",1,{"v":0.0048780487804878,"d":"0.5%"}]
["脱粒机",3,{"v":0.0146341463414634,"d":"1.5%"}]
["脱蓬（脯）机",7,{"v":0.0341463414634146,"d":"3.4%"}]
["微喷灌设备",2,{"v":0.00975609756097561,"d":"1.0%"}]
["喂（送）料机",4,{"v":0.0195121951219512,"d":"2.0%"}]
["移栽机",10,{"v":0.0487804878048781,"d":"4.9%"}]
["油菜籽干燥机",5,{"v":0.024390243902439,"d":"2.4%"}]
["油料果（籽）脱（剥）壳机",4,{"v":0.0195121951219512,"d":"2.0%"}]
["玉米收获专用割台",2,{"v":0.00975609756097561,"d":"1.0%"}]
["育秧（苗）播种设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["沼液沼渣抽排设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["枝条切碎机",2,{"v":0.00975609756097561,"d":"1.0%"}]
["中耕机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["种子包衣机",2,{"v":0.00975609756097561,"d":"1.0%"}]
["种子催芽机",1,{"v":0.0048780487804878,"d":"0.5%"}]
["种子清选机",5,{"v":0.024390243902439,"d":"2.4%"}]

{"sheet":"37个小类","index":3,"n_rows":38,"n_cols":3,"rows_kept":38}
["列C","计数","占比"]
["病死畜禽储运及处理设备",7,{"v":0.0341463414634146,"d":"3.4%"}]
["播种机械（可含施肥功能）",3,{"v":0.0146341463414634,"d":"1.5%"}]
["茶叶初加工机械",13,{"v":0.0634146341463415,"d":"6.3%"}]
["畜禽粪污资源化利用设备",34,{"v":0.165853658536585,"d":"16.6%"}]
["耕地机械",2,{"v":0.00975609756097561,"d":"1.0%"}]
["耕整地播种作业机械（可含施肥功能）",4,{"v":0.0195121951219512,"d":"2.0%"}]
["果菜茶烟草药收获机械",3,{"v":0.0146341463414634,"d":"1.5%"}]
["果蔬初加工机械",15,{"v":0.0731707317073171,"d":"7.3%"}]
["粮食初加工机械",9,{"v":0.0439024390243902,"d":"4.4%"}]
["粮食作物收获机械",3,{"v":0.0146341463414634,"d":"1.5%"}]
["农田废弃物收集设备",6,{"v":0.0292682926829268,"d":"2.9%"}]
["农作物废弃物处理设备",10,{"v":0.0487804878048781,"d":"4.9%"}]
["喷灌机械",6,{"v":0.0292682926829268,"d":"2.9%"}]
["清理机械",1,{"v":0.0048780487804878,"d":"0.5%"}]
["施肥机械",1,{"v":0.0048780487804878,"d":"0.5%"}]
["食用菌生产设备",5,{"v":0.024390243902439,"d":"2.4%"}]
["收获割台",2,{"v":0.00975609756097561,"d":"1.0%"}]
["水质调控设备",1,{"v":0.0048780487804878,"d":"0.5%"}]
["饲料（草）搬运机械",2,{"v":0.00975609756097561,"d":"1.0%"}]
["饲料（草）加工机械",5,{"v":0.024390243902439,"d":"2.4%"}]
["饲料（草）收获机械",8,{"v":0.0390243902439024,"d":"3.9%"}]
["饲养设备",4,{"v":0.0195121951219512,"d":"2.0%"}]
["糖料初加工机械",1,{"v":0.0048780487804878,"d":"0.5%"}]
["糖料作物收获机械",4,{"v":0.0195121951219512,"d":"2.0%"}]
["天然橡胶初加工机械",3,{"v":0.0146341463414634,"d":"1.5%"}]
["天然橡胶收获机械",1,{"v":0.0048780487804878,"d":"0.5%"}]
["田间作业监控设备",2,{"v":0.00975609756097561,"d":"1.0%"}]
["拖拉机",2,{"v":0.00975609756097561,"d":"1.0%"}]
["微灌设备",2,{"v":0.00975609756097561,"d":"1.0%"}]
["修剪防护管理机械",3,{"v":0.0146341463414634,"d":"1.5%"}]
["油料初加工机械",11,{"v":0.0536585365853659,"d":"5.4%"}]
["栽植机械",11,{"v":0.0536585365853659,"d":"5.4%"}]
["整地机械",4,{"v":0.0195121951219512,"d":"2.0%"}]
["植保机械",6,{"v":0.0292682926829268,"d":"2.9%"}]
["中耕机械",1,{"v":0.0048780487804878,"d":"0.5%"}]
["种子播前处理和育苗机械设备",2,{"v":0.00975609756097561,"d":"1.0%"}]
["种子初加工机械",7,{"v":0.0341463414634146,"d":"3.4%"}]

{"sheet":"18个大类","index":4,"n_rows":19,"n_cols":3,"rows_kept":19}
["列B","计数","占比"]
["畜禽养殖废弃物及病死畜禽处理设备",41,{"v":0.2,"d":"20.0%"}]
["畜禽养殖机械",4,{"v":0.0195121951219512,"d":"2.0%"}]
["耕整地机械",6,{"v":0.0292682926829268,"d":"2.9%"}]
["灌溉机械",8,{"v":0.0390243902439024,"d":"3.9%"}]
["果菜茶初加工机械",28,{"v":0.136585365853659,"d":"13.7%"}]
["粮油糖初加工机械",21,{"v":0.102439024390244,"d":"10.2%"}]
["农田基本建设机械",1,{"v":0.0048780487804878,"d":"0.5%"}]
["农用动力机械",2,{"v":0.00975609756097561,"d":"1.0%"}]
["设施种植机械",5,{"v":0.024390243902439,"d":"2.4%"}]
["收获机械",13,{"v":0.0634146341463415,"d":"6.3%"}]
["水产养殖机械",1,{"v":0.0048780487804878,"d":"0.5%"}]
["饲料（草）收获加工运输设备",15,{"v":0.0731707317073171,"d":"7.3%"}]
["天然橡胶初加工机械",3,{"v":0.0146341463414634,"d":"1.5%"}]
["田间管理机械",10,{"v":0.0487804878048781,"d":"4.9%"}]
["田间监测及作业监控设备",2,{"v":0.00975609756097561,"d":"1.0%"}]
["种植施肥机械",21,{"v":0.102439024390244,"d":"10.2%"}]
["种植业废弃物处理设备",16,{"v":0.0780487804878049,"d":"7.8%"}]
["种子初加工机械",7,{"v":0.0341463414634146,"d":"3.4%"}]